{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Absorption"],"not_rendered":{"charts":1,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Absorption","index":0,"n_rows":44,"n_cols":16,"rows_kept":44,"cut":false,"hidden":false,"merged":[[28,2,28,3],[1,2,1,10],[21,8,21,10],[41,8,41,10],[21,4,21,6],[41,4,41,6],[2,16,2,18],[4,2,4,6],[10,2,10,6],[4,8,4,10],[10,8,10,10]]}
[]
[null,null,"Modificar células com fundo branco só!"]
[]
[]
[null,null,"Características da fase gás",null,null,null,null,null,"Características da coluna"]
[null,null,"Pressão parcial de CO2",0.89,"bar",{"$f":"D6*100000","v":89000},"Pa",null,"Diâmetro",0.05,"m"]
[null,null,"Vazão de gás",100,"mL/min",{"$f":"(D7*0.000001)/60","v":1.6666666666666665E-6},"m3/s",null,"Altura do leito",0.65,"m"]
[null,null,"Vazão molar de gás",{"$f":"F7*(1000/24.4)","v":6.8306010928961749E-5},"mole/s",null,null,null,"Seção transversal",{"$f":"(PI()/4)*J6^2","v":1.9634954084936209E-3},"m2"]
[]
[]
[null,null,"Características da fase líquida",null,null,null,null,null,"Dados fisico-químicos"]
[null,null,"Vazão de líquido",20,"ml/min",{"$f":"D12*(0.000001/60)","v":3.3333333333333335E-7},"m3/s",null,"Coeficiente de difusão do CO2",1.8E-9,"m2/s"]
[null,null,"Concentração de NaOH no topo",0.1,"mole/L",{"$f":"D13*1000","v":100},"mole/m3",null,"CO2 Henry constant",3039,"Pa·m3/mole"]
[null,null,"Concentração de NaOH no fundo",4.19E-2,"mole/L",{"$f":"D14*1000","v":41.9},"mole/m3",null,"NaOH diffusion coefficient",3.0600000000000002E-9,"m2/s"]
[null,null,"Concentração total no líquido",55.56,"mole/L",{"$f":"D15*1000","v":55560},"mole/m3"]
[null,null,"Vazão molar de inerte no líquido",{"$f":"D12*0.001*D15","v":1.1112},"mole/min",{"$f":"D16/60","v":1.8519999999999998E-2},"mole/s"]
[null,null,"Velocidade mássica do líquido",{"$f":"((F16*(18/1000))/J8)","v":0.16977885385316549},"Kg/m2·s"]
[]
[]
[]
[]
[null,null,null,null,"GÁS: SAÍDA",null,null,null,"LÍQUIDO: ENTRADA"]
[null,null,null,null,"Vazão de gás",{"$f":"F43-(J43/(2*F15))*(J24-J44)","v":5.8622677595628419E-5},"mole/s",null,"Vazão de líquido inerte",{"$f":"F16","v":1.8519999999999998E-2},"mole/s"]
[null,null,null,null,"Pressão parcial de CO2",{"$f":"0.88*101300","v":89144},"Pa",null,"Concentração de NaOH",{"$f":"F13","v":100},"mole/m3"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Nó","Posição / m","CNaOH/mol/m3","CO2 removido / ml/min"]
[null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"$J$7*(M26/15)","v":0},{"$f":"F13","v":100},{"$f":"(($F$16/(2*$F$15))*(O26-$O$41))*60*24420","v":14.188019998383798}]
[null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"$J$7*(M27/15)","v":4.3333333333333335E-2},94.365734209309352,12.812132292297141]
[null,null,null,null,null,null,null,null,null,null,null,null,2,8.666666666666667E-2,89.048916693374323,11.513765454905805]
[null,null,"DADOS A CALCULAR",null,null,null,null,null,null,null,null,null,3,0.13,84.031661648588937,10.288551772969216]
[null,null,"kl·a / s-1",{"$f":"((F16*J12)/(J8*F15*J14*J7))*LN((2*J12+J13*J14*F13)/(2*J12+J13*J14*F14))","v":1.336427548231782E-4},null,null,null,null,null,null,null,null,4,0.17333333333333334,79.297090994437156,9.132369619225349]
[null,null,"kl·a / h-1",{"$f":"D30*3600","v":0.4811139173634415},null,null,null,null,null,null,null,null,5,0.21666666666666667,74.82927760263938,8.0413295889483329]
[null,null,null,null,null,null,null,null,null,null,null,null,6,0.26,70.613191718183259,7.0117614159641484]
[null,null,null,null,null,null,null,null,null,null,null,null,7,0.30333333333333334,66.634650399124382,6.0402016258499707]
[null,null,null,null,null,null,null,null,null,null,null,null,8,0.34666666666666668,62.880269805071919,5.1233818847823596]
[null,null,null,null,null,null,null,null,null,null,null,null,9,0.39,59.337420173857353,4.2582180048397626]
[null,null,null,null,null,null,null,null,null,null,null,null,10,0.43333333333333335,55.994183334927619,3.441799568773122]
[null,null,null,null,null,null,null,null,null,null,null,null,11,0.47666666666666663,52.839312616537313,2.671380139342209]
[null,null,null,null,null,null,null,null,null,null,null,null,12,0.52,49.862195011867449,1.9443680202818285]
[null,null,null,null,null,null,null,null,null,null,null,null,13,0.56333333333333335,47.052815476797548,1.2583175378177587]
[null,null,null,null,null,null,null,null,null,null,null,null,14,0.60666666666666669,44.401723239228104,0.61092081340330051]
[null,null,null,null,null,null,null,null,null,null,null,null,15,0.65,41.900000006618356,{"$f":"(($F$16/(2*$F$15))*(O41-$O$41))*60*24420","v":0}]
[null,null,null,null,"GÁS: ENTRADA",null,null,null,"LÍQUIDO: SAÍDA"]
[null,null,null,null,"Vazão de gás",{"$f":"D8","v":6.8306010928961749E-5},"mole/s",null,"Vazão de líquido inerte",{"$f":"F16","v":1.8519999999999998E-2},"mole/s"]
[null,null,null,null,"Pressão parcial de CO2",{"$f":"0.88*101300","v":89144},"Pa",null,"Concentração de NaOH",{"$f":"F14","v":41.9},"mole/m3"]